DECODE3-CTRL3: RESET initial mode is   #00000033                                
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa   #00000008                      
DECODE3-CTRL3: Received from OP register...Opb   #000000B8                      
DECODE3-CTRL3: Waiting from DEC3...    #00000000                                
DECODE3-CTRL3: Received from DEC3...    #00000000                               
DECODE3-CTRL3: waiting for CPSR   #00000000                                     
DECODE3-CTRL3: received CPSR   #00000000                                        
DECODE3-CTRL3: newpass is   #00000000                                           
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000073                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000000C0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #0000049F                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F68FF                                 
DECODE3-DEC3: AluC output is   #01BB9D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F68FF                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000000                       
DECODE3-CTRL3: Received from OP register...Opb   #0000C000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03C4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000073                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #0000C000                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BDF                                 
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FC9B3                                 
DECODE3-DEC3: AluC output is   #01BB45FF                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FC9B3                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03CA1BFF                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000000CC                       
DECODE3-CTRL3: Received from OP register...Opb   #00000010                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03CA1BFF                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000001                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: Waiting to send ALUgo to Dec1   #00000000                        
DECODE3-CTRL3: ALUgo sent to Dec1   #00000000                                   
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000000D0                       
DECODE3-CTRL3: Received from OP register...Opb   #00000010                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000000E0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F687F                                 
DECODE3-DEC3: AluC output is   #01BB9D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F687F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000000                       
DECODE3-CTRL3: Received from OP register...Opb   #F0000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03C4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #0000000A                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #F0000000                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BFE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F687F                                 
DECODE3-DEC3: AluC output is   #01BB9D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F687F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #F0000000                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03C4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000004                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000000                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BFE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FCAB3                                 
DECODE3-DEC3: AluC output is   #01BB45FF                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FCAB3                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03D21BFF                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000000F0                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03D21BFF                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000004                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000004                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: Waiting to send ALUgo to Dec1   #00000000                        
DECODE3-CTRL3: ALUgo sent to Dec1   #00000000                                   
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000000F4                       
DECODE3-CTRL3: Received from OP register...Opb   #0000017C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000270                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000278                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000278                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000280                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFEA0                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000284                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFEB4                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000288                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000288                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000290                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000290                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000298                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFEE8                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #0000029C                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFEFC                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002A0                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002A0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002A8                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFF20                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002AC                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFF34                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002B0                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002B0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002B8                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFF58                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002BC                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002BC                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002C4                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002C4                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002CC                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFF8C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FCAB3                                 
DECODE3-DEC3: AluC output is   #01BB45FF                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FCAB3                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03D21BFF                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002D0                       
DECODE3-CTRL3: Received from OP register...Opb   #10000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03D21BFF                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000004                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: Waiting to send ALUgo to Dec1   #00000000                        
DECODE3-CTRL3: ALUgo sent to Dec1   #00000000                                   
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F207F                                 
DECODE3-DEC3: AluC output is   #00AF9D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F207F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000000                       
DECODE3-CTRL3: Received from OP register...Opb   #00000001                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000001                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BFE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002D8                       
DECODE3-CTRL3: Received from OP register...Opb   #00000004                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002DC                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002E4                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFFFC                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000002E0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002E8                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFE38                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002EC                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFE4C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FBFF7                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FBFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF7D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000002F0                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFE60                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF7D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000150                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BF                                 
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FFFF7                                 
DECODE3-DEC3: AluC output is   #00AFEA96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FFFF7                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FF752E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-DEC3: Received In3 from DEC1  #000F7FCF                                 
DECODE3-DEC3: AluC output is   #012FFD7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F7FCF                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000097                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03FFFAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000158                       
DECODE3-CTRL3: Received from OP register...Opb   #FFFFFF10                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03FF752E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000068                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #000004BE                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-CTRL3: Received from OP register...Opa  #00000003                       
DECODE3-CTRL3: Received from OP register...Opb   #00000158                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000097                          
DECODE3-CTRL3: Received from Dec3... C3   #03FFFAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000154                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BFE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F727F                                 
DECODE3-DEC3: AluC output is   #00D79D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F727F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #0000006B                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03D4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000154                       
DECODE3-CTRL3: Received from OP register...Opb   #FC000003                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #0000006B                          
DECODE3-CTRL3: Received from Dec3... C3   #03D4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000154                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BFE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000E356D                                 
DECODE3-DEC3: AluC output is   #00AFFDD0                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000E356D                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03EFEBA8                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000154                       
DECODE3-CTRL3: Received from OP register...Opb   #00000001                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03EFEBA8                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: pass=TRUE,waiting to receive abort from memory  #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000155                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000EB4                                 
DECODE3-DEC3: Received In3 from DEC1  #000FCC7F                                 
DECODE3-DEC3: AluC output is   #00BD8096                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FCC7F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #0000005E                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03E4312E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: pass=TRUE, received Dabt0 from memory    #00000000               
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-CTRL3: Received from OP register...Opa  #00000042                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #0000005E                          
DECODE3-CTRL3: Received from Dec3... C3   #03E4312E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000008                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #0005C05B                                 
DECODE3-DEC3: AluC output is   #00FAAA96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #0005C05B                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #0000007D                                    
DECODE3-DEC3: sent to Ctrl3  C3  #0105552E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000008                       
DECODE3-CTRL3: Received from OP register...Opb   #0000007C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #0000007D                          
DECODE3-CTRL3: Received from Dec3... C3   #0105552E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000002                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000008                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #0000049F                                 
DECODE3-CTRL3: Waiting to send ALUgo to Dec1   #00000000                        
DECODE3-CTRL3: ALUgo sent to Dec1   #00000000                                   
DECODE3-CTRL3: PCpar has changed....   #00000000                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000001                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #00054057                                 
DECODE3-DEC3: AluC output is   #00FBF97F                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #00054057                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #0000007D                                    
DECODE3-DEC3: sent to Ctrl3  C3  #0147F2FF                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-DEC3: Received In3 from DEC1  #00054047                                 
DECODE3-DEC3: AluC output is   #012FFD7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #00054047                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000097                                    
DECODE3-DEC3: sent to Ctrl3  C3  #0147FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #0000007C                       
DECODE3-CTRL3: Received from OP register...Opb   #0000007C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #0000007D                          
DECODE3-CTRL3: Received from Dec3... C3   #0147F2FF                             
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000010                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000010                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00001BFF                                 
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-CTRL3: Received from OP register...Opa  #00000003                       
DECODE3-CTRL3: Received from OP register...Opb   #0000007C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000097                          
DECODE3-CTRL3: Received from Dec3... C3   #0147FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000002                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000078                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BDF                                 
DECODE3-CTRL3: PCpar not sent....   #00000001                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F8077                                 
DECODE3-DEC3: AluC output is   #00AFEE96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F8077                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C77D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000010                       
DECODE3-CTRL3: Received from OP register...Opb   #00000090                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03C77D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000000A0                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #0000049E                                 
DECODE3-CTRL3: PCpar has changed....   #00000001                                
DECODE3-CTRL3: PCpar sent to Dec1....   #00000000                               
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F047F                                 
DECODE3-DEC3: AluC output is   #00B79D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F047F                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #0000005B                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03E4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000042                       
DECODE3-CTRL3: Received from OP register...Opb   #000000FF                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #0000005B                          
DECODE3-CTRL3: Received from Dec3... C3   #03E4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000008                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #00000042                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BDE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FE8FF                                 
DECODE3-DEC3: AluC output is   #01BB8E96                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FE8FF                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C47D2E                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #00000042                       
DECODE3-CTRL3: Received from OP register...Opb   #00000078                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03C47D2E                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000FE3ED                                 
DECODE3-DEC3: AluC output is   #00AFFC88                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000FE3ED                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03DFE918                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #000000B0                       
DECODE3-CTRL3: Received from OP register...Opb   #0000000C                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03DFE918                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: pass=TRUE,waiting to receive abort from memory  #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #000000BC                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000454                                 
DECODE3-DEC3: Received In3 from DEC1  #000F68FF                                 
DECODE3-DEC3: AluC output is   #01BB9D7E                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F68FF                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #000000DD                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03C4FAFE                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: pass=TRUE, received Dabt0 from memory    #00000000               
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-CTRL3: Received from OP register...Opa  #00000042                       
DECODE3-CTRL3: Received from OP register...Opb   #0000C000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #000000DD                          
DECODE3-CTRL3: Received from Dec3... C3   #03C4FAFE                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: C3[12] is TRUE, not reading Dabt from memory    #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #0000C000                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000BDE                                 
DECODE3-CTRL3: PCpar not sent....   #00000000                                   
DECODE3-CTRL3: Waiting from OP register...    #00000000                         
DECODE3-DEC3: Received In3 from DEC1  #000F336D                                 
DECODE3-DEC3: AluC output is   #00AFFDC8                                        
DECODE3-DEC3: Waiting to send to Ctrl3   #000F336D                              
DECODE3-DEC3: sent to Ctrl3 ALfs   #00000057                                    
DECODE3-DEC3: sent to Ctrl3  C3  #03DFEB98                                      
DECODE3-DEC3: waiting for In3 from DEC1  #00000000                              
DECODE3-CTRL3: Received from OP register...Opa  #0000C000                       
DECODE3-CTRL3: Received from OP register...Opb   #00000000                      
DECODE3-CTRL3: Waiting from Dec3...    #00000000                                
DECODE3-CTRL3: Received from Dec3... ALfs    #00000057                          
DECODE3-CTRL3: Received from Dec3... C3   #03DFEB98                             
DECODE3-CTRL3: Waiting from CPSR register...    #00000000                       
DECODE3-CTRL3: Received from CPSR register...    #00000000                      
DECODE3-CTRL3: pass=TRUE,waiting to receive abort from memory  #00000000        
DECODE3-CTRL3: Output of CPmx   #00000000                                       
DECODE3-CTRL3: calling ALU  new flags are   #00000000                           
DECODE3-CTRL3: new CP2 is    #00000053                                          
DECODE3-CTRL3: waiting to send to WrtCtrl   #00000000                           
DECODE3-CTRL3: sent to WrtCtrl  RE   #0000C000                                  
DECODE3-CTRL3: sent to WrtCtrl  alP   #00000E54                                 
