*
* To combine C programs and assembler to run on the ASIM model
*

    The C source must be complied down to assembler:

	armcc (-pcc) -S xxxx.c

    (Note: Cannot go straight to object code
                         since we must change the byte-order)


   Then assemble, swapping the byte-order:

	armasm -LI -o xxxx xxxx.s


    Assemble the ASIM model 'wrapper':

	armasm -LI -PD "AsimVersion SETA 1" -o wrap wrapper.s


    Link all the object files to produce a plain binary:

	armlink -o binfile -BIN wrap xxxx yyyy zzzz
